{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["台账管理相机数据"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"台账管理相机数据","index":0,"n_rows":2,"n_cols":13,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["相机编码","通道编号","所属工务段编码(单位id)","行别","监控相机安装里程位置","监控范围开始里程位置","监控范围结束里程位置","监视相机经度","监视相机纬度","线路编码","物联网卡号","是否开启录像","录像接口返回的任务ID"]
["34020000001320000002","34020000001320000002","100","上行","8104","18","25","25.6","236","1244001","12346","否","34020000001320000002/34020000001320000002/flv/temp-20230310124549"]